; J9775A Configuration Editor; Created on release #YA.16.06.0006
; Ver #13:44.00.04.19.02.13.98.82.34.61.18.28.f3.84.9c.63.ff.37.27:43
hostname "SW-P3-RdosenInfor-2530-48"
mirror-port 2
ip default-gateway 192.168.161.1
interface 1
monitor
exit
interface 5
monitor
exit
snmp-server community "public" unrestricted
vlan 1
name "DEFAULT_VLAN"
no untagged 1-48
untagged 49-52
ip address dhcp-bootp
exit
vlan 100
name "VLAN100"
tagged 47
no ip address
exit
vlan 120
name "VLAN120"
untagged 47-48
ip address 192.168.161.215 255.255.255.0
exit
vlan 914
name "VLAN914"
untagged 13-24
tagged 48
no ip address
exit
vlan 921
name "VLAN921"
untagged 1-12,25-46
tagged 48
no ip address
exit
spanning-tree
no tftp server
no dhcp config-file-update
no dhcp image-file-update
no dhcp tr69-acs-url
password manager
password operator
