%YAML 1.1
---

# Suricata configuration file. In addition to the comments describing all
# options in this file, full documentation can be found at:
# https://docs.suricata.io/en/latest/configuration/suricata-yaml.html

# This configuration file generated by Suricata 7.0.8.
suricata-version: "7.0"

##
## Step 1: Inform Suricata about your network
##

vars:
  # more specific is better for alert accuracy and performance
  address-groups:
    HOME_NET: "[192.168.156.0/24,192.168.160.0/24,192.168.104.0/21]"
    #HOME_NET: "[192.168.0.0/16]"
    #HOME_NET: "[10.0.0.0/8]"
    #HOME_NET: "[172.16.0.0/12]"
    #HOME_NET: "any"

    EXTERNAL_NET: "!$HOME_NET"
    #EXTERNAL_NET: "any"

    HTTP_SERVERS: "$HOME_NET"
    SMTP_SERVERS: "$HOME_NET"
    SQL_SERVERS: "$HOME_NET"
    DNS_SERVERS: "$HOME_NET"
    TELNET_SERVERS: "$HOME_NET"
    AIM_SERVERS: "$EXTERNAL_NET"
    DC_SERVERS: "$HOME_NET"
    DNP3_SERVER: "$HOME_NET"
    DNP3_CLIENT: "$HOME_NET"
    MODBUS_CLIENT: "$HOME_NET"
    MODBUS_SERVER: "$HOME_NET"
    ENIP_CLIENT: "$HOME_NET"
    ENIP_SERVER: "$HOME_NET"

  port-groups:
    HTTP_PORTS: "80"
    SHELLCODE_PORTS: "!80"
    ORACLE_PORTS: 1521
    SSH_PORTS: 22
    DNP3_PORTS: 20000
    MODBUS_PORTS: 502
    FILE_DATA_PORTS: "[$HTTP_PORTS,110,143]"
    FTP_PORTS: 21
    GENEVE_PORTS: 6081
    VXLAN_PORTS: 4789
    TEREDO_PORTS: 3544

##
## Step 2: Select outputs to enable
##

# The default logging directory.  Any log or output file will be
# placed here if it's not specified with a full path name. This can be
# overridden with the -l command line parameter.
default-log-dir: /var/log/suricata/

# Global stats configuration
stats:
  enabled: yes
  # The interval field (in seconds) controls the interval at
  # which stats are updated in the log.
  interval: 8
  # Add decode events to stats.
  #decoder-events: true
  # Decoder event prefix in stats. Has been 'decoder' before, but that leads
  # to missing events in the eve.stats records. See issue #2225.
  #decoder-events-prefix: "decoder.event"
  # Add stream events as stats.
  #stream-events: false

# Plugins -- Experimental -- specify the filename for each plugin shared object
plugins:
#   - /path/to/plugin.so

# Configure the type of alert (and other) logging you would like.
outputs:
  # a line based alerts log similar to Snort's fast.log
  - fast:
      enabled: yes
      filename: fast.log
      append: yes
      #filetype: regular # 'regular', 'unix_stream' or 'unix_dgram'

  # Extensible Event Format (nicknamed EVE) event log in JSON format
  - eve-log:
      enabled: yes
      filetype: regular #regular|syslog|unix_dgram|unix_stream|redis
      filename: eve.json
      # Enable for multi-threaded eve.json output; output files are amended with
      # an identifier, e.g., eve.9.json
      #threaded: false
      #prefix: "@cee: " # prefix to prepend to each log entry
      # the following are valid when type: syslog above
      #identity: "suricata"
      #facility: local5
      #level: Info ## possible levels: Emergency, Alert, Critical,
                   ## Error, Warning, Notice, Info, Debug
      #ethernet: no  # log ethernet header in events when available
      #redis:
      #  server: 127.0.0.1
      #  port: 6379
      #  async: true ## if redis replies are read asynchronously
      #  mode: list ## possible values: list|lpush (default), rpush, channel|publish
      #             ## lpush and rpush are using a Redis list. "list" is an alias for lpush
      #             ## publish is using a Redis channel. "channel" is an alias for publish
      #  key: suricata ## key or channel to use (default to suricata)
      # Redis pipelining set up. This will enable to only do a query every
      # 'batch-size' events. This should lower the latency induced by network
      # connection at the cost of some memory. There is no flushing implemented
      # so this setting should be reserved to high traffic Suricata deployments.
      #  pipelining:
      #    enabled: yes ## set enable to yes to enable query pipelining
      #    batch-size: 10 ## number of entries to keep in buffer

      # Include top level metadata. Default yes.
      #metadata: no

      # include the name of the input pcap file in pcap file processing mode
      pcap-file: false

      # Community Flow ID
      # Adds a 'community_id' field to EVE records. These are meant to give
      # records a predictable flow ID that can be used to match records to
      # output of other tools such as Zeek (Bro).
      #
      # Takes a 'seed' that needs to be same across sensors and tools
      # to make the id less predictable.

      # enable/disable the community id feature.
      community-id: false
      # Seed value for the ID output. Valid values are 0-65535.
      community-id-seed: 0

      # HTTP X-Forwarded-For support by adding an extra field or overwriting
      # the source or destination IP address (depending on flow direction)
      # with the one reported in the X-Forwarded-For HTTP header. This is
      # helpful when reviewing alerts for traffic that is being reverse
      # or forward proxied.
      xff:
        enabled: no
        # Two operation modes are available: "extra-data" and "overwrite".
        mode: extra-data
        # Two proxy deployments are supported: "reverse" and "forward". In
        # a "reverse" deployment the IP address used is the last one, in a
        # "forward" deployment the first IP address is used.
        deployment: reverse
        # Header name where the actual IP address will be reported. If more
        # than one IP address is present, the last IP address will be the
        # one taken into consideration.
        header: X-Forwarded-For

      types:
        - alert:
            # payload: yes             # enable dumping payload in Base64
            # payload-buffer-size: 4kb # max size of payload buffer to output in eve-log
            # payload-printable: yes   # enable dumping payload in printable (lossy) format
            # packet: yes              # enable dumping of packet (without stream segments)
            # metadata: no             # enable inclusion of app layer metadata with alert. Default yes
            # http-body: yes           # Requires metadata; enable dumping of HTTP body in Base64
            # http-body-printable: yes # Requires metadata; enable dumping of HTTP body in printable format

            # Enable the logging of tagged packets for rules using the
            # "tag" keyword.
            tagged-packets: yes
            # Enable logging the final action taken on a packet by the engine
            # (e.g: the alert may have action 'allowed' but the verdict be
            # 'drop' due to another alert. That's the engine's verdict)
            # verdict: yes
        # app layer frames
        - frame:
            # disabled by default as this is very verbose.
            enabled: no
            # payload-buffer-size: 4kb # max size of frame payload buffer to output in eve-log
        - anomaly:
            # Anomaly log records describe unexpected conditions such
            # as truncated packets, packets with invalid IP/UDP/TCP
            # length values, and other events that render the packet
            # invalid for further processing or describe unexpected
            # behavior on an established stream. Networks which
            # experience high occurrences of anomalies may experience
            # packet processing degradation.
            #
            # Anomalies are reported for the following:
            # 1. Decode: Values and conditions that are detected while
            # decoding individual packets. This includes invalid or
            # unexpected values for low-level protocol lengths as well
            # as stream related events (TCP 3-way handshake issues,
            # unexpected sequence number, etc).
            # 2. Stream: This includes stream related events (TCP
            # 3-way handshake issues, unexpected sequence number,
            # etc).
            # 3. Application layer: These denote application layer
            # specific conditions that are unexpected, invalid or are
            # unexpected given the application monitoring state.
            #
            # By default, anomaly logging is enabled. When anomaly
            # logging is enabled, applayer anomaly reporting is
            # also enabled.
            enabled: yes
            #
            # Choose one or more types of anomaly logging and whether to enable
            # logging of the packet header for packet anomalies.
            types:
              # decode: no
              # stream: no
              # applayer: yes
            #packethdr: no
        - http:
            extended: yes     # enable this for extended logging information
            # custom allows additional HTTP fields to be included in eve-log.
            # the example below adds three additional fields when uncommented
            #custom: [Accept-Encoding, Accept-Language, Authorization]
            # set this value to one and only one from {both, request, response}
            # to dump all HTTP headers for every HTTP request and/or response
            # dump-all-headers: none
        #- dns:
            # This configuration uses the new DNS logging format,
            # the old configuration is still available:
            # https://docs.suricata.io/en/latest/output/eve/eve-json-output.html#dns-v1-format

            # As of Suricata 5.0, version 2 of the eve dns output
            # format is the default.
            #version: 2

            # Enable/disable this logger. Default: enabled.
            #enabled: yes

            # Control logging of requests and responses:
            # - requests: enable logging of DNS queries
            # - responses: enable logging of DNS answers
            # By default both requests and responses are logged.
            #requests: no
            #responses: no

            # Format of answer logging:
            # - detailed: array item per answer
            # - grouped: answers aggregated by type
            # Default: all
            #formats: [detailed, grouped]

            # DNS record types to log, based on the query type.
            # Default: all.
            #types: [a, aaaa, cname, mx, ns, ptr, txt]
        - tls:
            extended: yes     # enable this for extended logging information
            # output TLS transaction where the session is resumed using a
            # session id
            #session-resumption: no
            # ja4 hashes in tls records will never be logged unless
            # the following is set to on. (Default off)
            # ja4: off
            # custom controls which TLS fields that are included in eve-log
            #custom: [subject, issuer, session_resumed, serial, fingerprint, sni, version, not_before, not_after, certificate, chain, ja3, ja3s, ja4]
        - files:
            force-magic: no   # force logging magic on all logged files
            # force logging of checksums, available hash functions are md5,
            # sha1 and sha256
            #force-hash: [md5]
        #- drop:
        #    alerts: yes      # log alerts that caused drops
        #    flows: all       # start or all: 'start' logs only a single drop
        #                     # per flow direction. All logs each dropped pkt.
            # Enable logging the final action taken on a packet by the engine
            # (will show more information in case of a drop caused by 'reject')
            # verdict: yes
        - smtp:
            #extended: yes # enable this for extended logging information
            # this includes: bcc, message-id, subject, x_mailer, user-agent
            # custom fields logging from the list:
            #  reply-to, bcc, message-id, subject, x-mailer, user-agent, received,
            #  x-originating-ip, in-reply-to, references, importance, priority,
            #  sensitivity, organization, content-md5, date
            #custom: [received, x-mailer, x-originating-ip, relays, reply-to, bcc]
            # output md5 of fields: body, subject
            # for the body you need to set app-layer.protocols.smtp.mime.body-md5
            # to yes
            #md5: [body, subject]

        #- dnp3
        - ftp
        - rdp
        - nfs
        - smb
        - tftp
        - ike
        - dcerpc
        - krb5
        - bittorrent-dht
        - snmp
        - rfb
        - sip
        - quic:
            # ja4 hashes in quic records will never be logged unless
            # the following is set to on. (Default off)
            # ja4: off
        - dhcp:
            enabled: yes
            # When extended mode is on, all DHCP messages are logged
            # with full detail. When extended mode is off (the
            # default), just enough information to map a MAC address
            # to an IP address is logged.
            extended: no
        - ssh
        - mqtt:
            # passwords: yes           # enable output of passwords
        - http2
        - pgsql:
            enabled: no
            # passwords: yes           # enable output of passwords. Disabled by default
        - stats:
            totals: yes       # stats for all threads merged together
            threads: no       # per thread stats
            deltas: no        # include delta values
        # bi-directional flows
        #- flow
        # uni-directional flows
        #- netflow

        # Metadata event type. Triggered whenever a pktvar is saved
        # and will include the pktvars, flowvars, flowbits and
        # flowints.
        #- metadata

        # EXPERIMENTAL per packet output giving TCP state tracking details
        # including internal state, flags, etc.
        # This output is experimental, meant for debugging and subject to
        # change in both config and output without any notice.
        #- stream:
        #   all: false                      # log all TCP packets
        #   event-set: false                # log packets that have a decoder/stream event
        #   state-update: false             # log packets triggering a TCP state update
        #   spurious-retransmission: false  # log spurious retransmission packets

  # a line based log of HTTP requests (no alerts)
  - http-log:
      enabled: no
      filename: http.log
      append: yes
      #extended: yes     # enable this for extended logging information
      #custom: yes       # enable the custom logging format (defined by customformat)
      #customformat: "%{%D-%H:%M:%S}t.%z %{X-Forwarded-For}i %H %m %h %u %s %B %a:%p -> %A:%P"
      #filetype: regular # 'regular', 'unix_stream' or 'unix_dgram'

  # a line based log of TLS handshake parameters (no alerts)
  - tls-log:
      enabled: no  # Log TLS connections.
      filename: tls.log # File to store TLS logs.
      append: yes
      #extended: yes     # Log extended information like fingerprint
      #custom: yes       # enabled the custom logging format (defined by customformat)
      #customformat: "%{%D-%H:%M:%S}t.%z %a:%p -> %A:%P %v %n %d %D"
      #filetype: regular # 'regular', 'unix_stream' or 'unix_dgram'
      # output TLS transaction where the session is resumed using a
      # session id
      #session-resumption: no

  # output module to store certificates chain to disk
  - tls-store:
      enabled: no
      #certs-log-dir: certs # directory to store the certificates files

  # Packet log... log packets in pcap format. 3 modes of operation: "normal"
  # "multi" and "sguil".
  #
  # In normal mode a pcap file "filename" is created in the default-log-dir,
  # or as specified by "dir".
  # In multi mode, a file is created per thread. This will perform much
  # better, but will create multiple files where 'normal' would create one.
  # In multi mode the filename takes a few special variables:
  # - %n -- thread number
  # - %i -- thread id
  # - %t -- timestamp (secs or secs.usecs based on 'ts-format'
  # E.g. filename: pcap.%n.%t
  #
  # Note that it's possible to use directories, but the directories are not
  # created by Suricata. E.g. filename: pcaps/%n/log.%s will log into the
  # per thread directory.
  #
  # Also note that the limit and max-files settings are enforced per thread.
  # So the size limit when using 8 threads with 1000mb files and 2000 files
  # is: 8*1000*2000 ~ 16TiB.
  #
  # In Sguil mode "dir" indicates the base directory. In this base dir the
  # pcaps are created in the directory structure Sguil expects:
  #
  # $sguil-base-dir/YYYY-MM-DD/$filename.<timestamp>
  #
  # By default all packets are logged except:
  # - TCP streams beyond stream.reassembly.depth
  # - encrypted streams after the key exchange
  #
  - pcap-log:
      enabled: no
      filename: log.pcap

      # File size limit.  Can be specified in kb, mb, gb.  Just a number
      # is parsed as bytes.
      limit: 1000mb

      # If set to a value, ring buffer mode is enabled. Will keep maximum of
      # "max-files" of size "limit"
      max-files: 2000

      # Compression algorithm for pcap files. Possible values: none, lz4.
      # Enabling compression is incompatible with the sguil mode. Note also
      # that on Windows, enabling compression will *increase* disk I/O.
      compression: none

      # Further options for lz4 compression. The compression level can be set
      # to a value between 0 and 16, where higher values result in higher
      # compression.
      #lz4-checksum: no
      #lz4-level: 0

      mode: normal # normal, multi or sguil.

      # Directory to place pcap files. If not provided the default log
      # directory will be used. Required for "sguil" mode.
      #dir: /nsm_data/

      #ts-format: usec # sec or usec second format (default) is filename.sec usec is filename.sec.usec
      use-stream-depth: no #If set to "yes" packets seen after reaching stream inspection depth are ignored. "no" logs all packets
      honor-pass-rules: no # If set to "yes", flows in which a pass rule matched will stop being logged.
      # Use "all" to log all packets or use "alerts" to log only alerted packets and flows or "tag"
      # to log only flow tagged via the "tag" keyword
      #conditional: all

  # a full alert log containing much information for signature writers
  # or for investigating suspected false positives.
  - alert-debug:
      enabled: no
      filename: alert-debug.log
      append: yes
      #filetype: regular # 'regular', 'unix_stream' or 'unix_dgram'

  # Stats.log contains data from various counters of the Suricata engine.
  - stats:
      enabled: yes
      filename: stats.log
      append: yes       # append to file (yes) or overwrite it (no)
      totals: yes       # stats for all threads merged together
      threads: no       # per thread stats
      #null-values: yes  # print counters that have value 0. Default: no

  # a line based alerts log similar to fast.log into syslog
  - syslog:
      enabled: no
      # reported identity to syslog. If omitted the program name (usually
      # suricata) will be used.
      #identity: "suricata"
      facility: local5
      #level: Info ## possible levels: Emergency, Alert, Critical,
                   ## Error, Warning, Notice, Info, Debug

  # Output module for storing files on disk. Files are stored in
  # directory names consisting of the first 2 characters of the
  # SHA256 of the file. Each file is given its SHA256 as a filename.
  #
  # When a duplicate file is found, the timestamps on the existing file
  # are updated.
  #
  # Unlike the older filestore, metadata is not written by default
  # as each file should already have a "fileinfo" record in the
  # eve-log. If write-fileinfo is set to yes, then each file will have
  # one more associated .json files that consist of the fileinfo
  # record. A fileinfo file will be written for each occurrence of the
  # file seen using a filename suffix to ensure uniqueness.
  #
  # To prune the filestore directory see the "suricatactl filestore
  # prune" command which can delete files over a certain age.
  - file-store:
      version: 2
      enabled: yes

      # Set the directory for the filestore. Relative pathnames
      # are contained within the "default-log-dir".
      #dir: filestore

      # Write out a fileinfo record for each occurrence of a file.
      # Disabled by default as each occurrence is already logged
      # as a fileinfo record to the main eve-log.
      #write-fileinfo: yes

      # Force storing of all files. Default: no.
      #force-filestore: yes

      # Override the global stream-depth for sessions in which we want
      # to perform file extraction. Set to 0 for unlimited; otherwise,
      # must be greater than the global stream-depth value to be used.
      #stream-depth: 0

      # Uncomment the following variable to define how many files can
      # remain open for filestore by Suricata. Default value is 0 which
      # means files get closed after each write to the file.
      #max-open-files: 1000

      # Force logging of checksums: available hash functions are md5,
      # sha1 and sha256. Note that SHA256 is automatically forced by
      # the use of this output module as it uses the SHA256 as the
      # file naming scheme.
      #force-hash: [sha1, md5]
      # NOTE: X-Forwarded configuration is ignored if write-fileinfo is disabled
      # HTTP X-Forwarded-For support by adding an extra field or overwriting
      # the source or destination IP address (depending on flow direction)
      # with the one reported in the X-Forwarded-For HTTP header. This is
      # helpful when reviewing alerts for traffic that is being reverse
      # or forward proxied.
      xff:
        enabled: no
        # Two operation modes are available, "extra-data" and "overwrite".
        mode: extra-data
        # Two proxy deployments are supported, "reverse" and "forward". In
        # a "reverse" deployment the IP address used is the last one, in a
        # "forward" deployment the first IP address is used.
        deployment: reverse
        # Header name where the actual IP address will be reported. If more
        # than one IP address is present, the last IP address will be the
        # one taken into consideration.
        header: X-Forwarded-For

  # Log TCP data after stream normalization
  # Two types: file or dir:
  #     - file logs into a single logfile.
  #     - dir creates 2 files per TCP session and stores the raw TCP
  #            data into them.
  # Use 'both' to enable both file and dir modes.
  #
  # Note: limited by "stream.reassembly.depth"
  - tcp-data:
      enabled: no
      type: file
      filename: tcp-data.log

  # Log HTTP body data after normalization, de-chunking and unzipping.
  # Two types: file or dir.
  #     - file logs into a single logfile.
  #     - dir creates 2 files per HTTP session and stores the
  #           normalized data into them.
  # Use 'both' to enable both file and dir modes.
  #
  # Note: limited by the body limit settings
  - http-body-data:
      enabled: no
      type: file
      filename: http-data.log

  # Lua Output Support - execute lua script to generate alert and event
  # output.
  # Documented at:
  # https://docs.suricata.io/en/latest/output/lua-output.html
  - lua:
      enabled: no
      #scripts-dir: /etc/suricata/lua-output/
      scripts:
      #   - script1.lua

# Logging configuration.  This is not about logging IDS alerts/events, but
# output about what Suricata is doing, like startup messages, errors, etc.
logging:
  # The default log level: can be overridden in an output section.
  # Note that debug level logging will only be emitted if Suricata was
  # compiled with the --enable-debug configure option.
  #
  # This value is overridden by the SC_LOG_LEVEL env var.
  default-log-level: notice

  # The default output format.  Optional parameter, should default to
  # something reasonable if not provided.  Can be overridden in an
  # output section.  You can leave this out to get the default.
  #
  # This console log format value can be overridden by the SC_LOG_FORMAT env var.
  #default-log-format: "%D: %S: %M"
  #
  # For the pre-7.0 log format use:
  #default-log-format: "[%i] %t [%S] - (%f:%l) <%d> (%n) -- "

  # A regex to filter output.  Can be overridden in an output section.
  # Defaults to empty (no filter).
  #
  # This value is overridden by the SC_LOG_OP_FILTER env var.
  default-output-filter:

  # Requires libunwind to be available when Suricata is configured and built.
  # If a signal unexpectedly terminates Suricata, displays a brief diagnostic
  # message with the offending stacktrace if enabled.
  #stacktrace-on-signal: on

  # Define your logging outputs.  If none are defined, or they are all
  # disabled you will get the default: console output.
  outputs:
  - console:
      enabled: yes
      # type: json
  - file:
      enabled: yes
      level: info
      filename: suricata.log
      # format: "[%i - %m] %z %d: %S: %M"
      # type: json
  - syslog:
      enabled: no
      facility: local5
      format: "[%i] <%d> -- "
      # type: json


##
## Step 3: Configure common capture settings
##
## See "Advanced Capture Options" below for more options, including Netmap
## and PF_RING.
##

# Linux high speed capture support
af-packet:
  - interface: eth0
    # Number of receive threads. "auto" uses the number of cores
    #threads: auto
    # Default clusterid. AF_PACKET will load balance packets based on flow.
    cluster-id: 99
    # Default AF_PACKET cluster type. AF_PACKET can load balance per flow or per hash.
    # This is only supported for Linux kernel > 3.1
    # possible value are:
    #  * cluster_flow: all packets of a given flow are sent to the same socket
    #  * cluster_cpu: all packets treated in kernel by a CPU are sent to the same socket
    #  * cluster_qm: all packets linked by network card to a RSS queue are sent to the same
    #  socket. Requires at least Linux 3.14.
    #  * cluster_ebpf: eBPF file load balancing. See doc/userguide/capture-hardware/ebpf-xdp.rst for
    #  more info.
    # Recommended modes are cluster_flow on most boxes and cluster_cpu or cluster_qm on system
    # with capture card using RSS (requires cpu affinity tuning and system IRQ tuning)
    # cluster_rollover has been deprecated; if used, it'll be replaced with cluster_flow.
    cluster-type: cluster_flow
    # In some fragmentation cases, the hash can not be computed. If "defrag" is set
    # to yes, the kernel will do the needed defragmentation before sending the packets.
    defrag: yes
    # To use the ring feature of AF_PACKET, set 'use-mmap' to yes
    #use-mmap: yes
    # Lock memory map to avoid it being swapped. Be careful that over
    # subscribing could lock your system
    #mmap-locked: yes
    # Use tpacket_v3 capture mode, only active if use-mmap is true
    # Don't use it in IPS or TAP mode as it causes severe latency
    #tpacket-v3: yes
    # Ring size will be computed with respect to "max-pending-packets" and number
    # of threads. You can set manually the ring size in number of packets by setting
    # the following value. If you are using flow "cluster-type" and have really network
    # intensive single-flow you may want to set the "ring-size" independently of the number
    # of threads:
    #ring-size: 2048
    # Block size is used by tpacket_v3 only. It should set to a value high enough to contain
    # a decent number of packets. Size is in bytes so please consider your MTU. It should be
    # a power of 2 and it must be multiple of page size (usually 4096).
    #block-size: 32768
    # tpacket_v3 block timeout: an open block is passed to userspace if it is not
    # filled after block-timeout milliseconds.
    #block-timeout: 10
    # On busy systems, set it to yes to help recover from a packet drop
    # phase. This will result in some packets (at max a ring flush) not being inspected.
    #use-emergency-flush: yes
    # recv buffer size, increased value could improve performance
    # buffer-size: 32768
    # Set to yes to disable promiscuous mode
    # disable-promisc: no
    # Choose checksum verification mode for the interface. At the moment
    # of the capture, some packets may have an invalid checksum due to
    # the checksum computation being offloaded to the network card.
    # Possible values are:
    #  - kernel: use indication sent by kernel for each packet (default)
    #  - yes: checksum validation is forced
    #  - no: checksum validation is disabled
    #  - auto: Suricata uses a statistical approach to detect when
    #  checksum off-loading is used.
    # Warning: 'capture.checksum-validation' must be set to yes to have any validation
    #checksum-checks: kernel
    # BPF filter to apply to this interface. The pcap filter syntax applies here.
    #bpf-filter: port 80 or udp
    # You can use the following variables to activate AF_PACKET tap or IPS mode.
    # If copy-mode is set to ips or tap, the traffic coming to the current
    # interface will be copied to the copy-iface interface. If 'tap' is set, the
    # copy is complete. If 'ips' is set, the packet matching a 'drop' action
    # will not be copied.
    #copy-mode: ips
    #copy-iface: eth1
    #  For eBPF and XDP setup including bypass, filter and load balancing, please
    #  see doc/userguide/capture-hardware/ebpf-xdp.rst for more info.

  # Put default values here. These will be used for an interface that is not
  # in the list above.
  - interface: default
    #threads: auto
    #use-mmap: no
    #tpacket-v3: yes

#detect-engine:
  #- rule-reload: true

# Linux high speed af-xdp capture support
af-xdp:
  - interface: eth0
    # Number of receive threads. "auto" uses least between the number
    # of cores and RX queues
    #threads: auto
    #disable-promisc: false
    # XDP_DRV mode can be chosen when the driver supports XDP
    # XDP_SKB mode can be chosen when the driver does not support XDP
    # Possible values are:
    #  - drv: enable XDP_DRV mode
    #  - skb: enable XDP_SKB mode
    #  - none: disable (kernel in charge of applying mode)
    #force-xdp-mode: none
    # During socket binding the kernel will attempt zero-copy, if this
    # fails it will fallback to copy. If this fails, the bind fails.
    # The bind can be explicitly configured using the option below.
    # If configured, the bind will fail if not successful (no fallback).
    # Possible values are:
    #  - zero: enable zero-copy mode
    #  - copy: enable copy mode
    #  - none: disable (kernel in charge of applying mode)
    #force-bind-mode: none
    # Memory alignment mode can vary between two modes, aligned and
    # unaligned chunk modes. By default, aligned chunk mode is selected.
    # select 'yes' to enable unaligned chunk mode.
    # Note: unaligned chunk mode uses hugepages, so the required number
    # of pages must be available.
    #mem-unaligned: no
    # The following options configure the prefer-busy-polling socket
    # options. The polling time and budget can be edited here.
    # Possible values are:
    #  - yes: enable (default)
    #  - no: disable
    #enable-busy-poll: yes
    # busy-poll-time sets the approximate time in microseconds to busy
    # poll on a blocking receive when there is no data.
    #busy-poll-time: 20
    # busy-poll-budget is the budget allowed for packet batches
    #busy-poll-budget: 64
    # These two tunables are used to configure the Linux OS's NAPI
    # context. Their purpose is to defer enabling of interrupts and
    # instead schedule the NAPI context from a watchdog timer.
    # The softirq NAPI will exit early, allowing busy polling to be
    # performed. Successfully setting these tunables alongside busy-polling
    # should improve performance.
    # Defaults are:
    #gro-flush-timeout: 2000000
    #napi-defer-hard-irq: 2

dpdk:
  eal-params:
    proc-type: primary

  # DPDK capture support
  # RX queues (and TX queues in IPS mode) are assigned to cores in 1:1 ratio
  interfaces:
    - interface: 0000:3b:00.0 # PCIe address of the NIC port
      # Threading: possible values are either "auto" or number of threads
      # - auto takes all cores
      # in IPS mode it is required to specify the number of cores and the numbers on both interfaces must match
      threads: auto
      # interrupt-mode: false # true to switch to interrupt mode 
      promisc: true # promiscuous mode - capture all packets
      multicast: true # enables also detection on multicast packets
      checksum-checks: true # if Suricata should validate checksums
      checksum-checks-offload: true # if possible offload checksum validation to the NIC (saves Suricata resources)
      mtu: 1500 # Set MTU of the device in bytes
      # rss-hash-functions: 0x0 # advanced configuration option, use only if you use untested NIC card and experience RSS warnings,
      # For `rss-hash-functions` use hexadecimal 0x01ab format to specify RSS hash function flags - DumpRssFlags can help (you can see output if you use -vvv option during Suri startup)
      # setting auto to rss_hf sets the default RSS hash functions (based on IP addresses)

      # To approximately calculate required amount of space (in bytes) for interface's mempool: mempool-size * mtu
      # Make sure you have enough allocated hugepages.
      # The optimum size for the packet memory pool (in terms of memory usage) is power of two minus one: n = (2^q - 1)
      mempool-size: 65535 # The number of elements in the mbuf pool

      # Mempool cache size must be lower or equal to:
      #     - RTE_MEMPOOL_CACHE_MAX_SIZE (by default 512) and
      #     - "mempool-size / 1.5"
      # It is advised to choose cache_size to have "mempool-size modulo cache_size == 0".
      # If this is not the case, some elements will always stay in the pool and will never be used.
      # The cache can be disabled if the cache_size argument is set to 0, can be useful to avoid losing objects in cache
      # If the value is empty or set to "auto", Suricata will attempt to set cache size of the mempool to a value
      # that matches the previously mentioned recommendations
      mempool-cache-size: 257
      rx-descriptors: 1024
      tx-descriptors: 1024
      #
      # IPS mode for Suricata works in 3 modes - none, tap, ips
      # - none: IDS mode only - disables IPS functionality (does not further forward packets)
      # - tap: forwards all packets and generates alerts (omits DROP action) This is not DPDK TAP
      # - ips: the same as tap mode but it also drops packets that are flagged by rules to be dropped
      copy-mode: none
      copy-iface: none # or PCIe address of the second interface

    - interface: default
      threads: auto
      promisc: true
      multicast: true
      checksum-checks: true
      checksum-checks-offload: true
      mtu: 1500
      rss-hash-functions: auto
      mempool-size: 65535
      mempool-cache-size: 257
      rx-descriptors: 1024
      tx-descriptors: 1024
      copy-mode: none
      copy-iface: none


# Cross platform libpcap capture support
pcap:
  - interface: eth0
    # On Linux, pcap will try to use mmap'ed capture and will use "buffer-size"
    # as total memory used by the ring. So set this to something bigger
    # than 1% of your bandwidth.
    #buffer-size: 16777216
    #bpf-filter: "tcp and port 25"
    # Choose checksum verification mode for the interface. At the moment
    # of the capture, some packets may have an invalid checksum due to
    # the checksum computation being offloaded to the network card.
    # Possible values are:
    #  - yes: checksum validation is forced
    #  - no: checksum validation is disabled
    #  - auto: Suricata uses a statistical approach to detect when
    #  checksum off-loading is used. (default)
    # Warning: 'capture.checksum-validation' must be set to yes to have any validation
    #checksum-checks: auto
    # With some accelerator cards using a modified libpcap (like Myricom), you
    # may want to have the same number of capture threads as the number of capture
    # rings. In this case, set up the threads variable to N to start N threads
    # listening on the same interface.
    #threads: 16
    # set to no to disable promiscuous mode:
    #promisc: no
    # set snaplen, if not set it defaults to MTU if MTU can be known
    # via ioctl call and to full capture if not.
    #snaplen: 1518
  # Put default values here
  - interface: default
    #checksum-checks: auto

# Settings for reading pcap files
pcap-file:
  # Possible values are:
  #  - yes: checksum validation is forced
  #  - no: checksum validation is disabled
  #  - auto: Suricata uses a statistical approach to detect when
  #  checksum off-loading is used. (default)
  # Warning: 'checksum-validation' must be set to yes to have checksum tested
  checksum-checks: auto

# See "Advanced Capture Options" below for more options, including Netmap
# and PF_RING.


##
## Step 4: App Layer Protocol configuration
##

# Configure the app-layer parsers.
#
# The error-policy setting applies to all app-layer parsers. Values can be
# "drop-flow", "pass-flow", "bypass", "drop-packet", "pass-packet", "reject" or
# "ignore" (the default).
#
# The protocol's section details each protocol.
#
# The option "enabled" takes 3 values - "yes", "no", "detection-only".
# "yes" enables both detection and the parser, "no" disables both, and
# "detection-only" enables protocol detection only (parser disabled).
app-layer:
  # error-policy: ignore
  protocols:
    telnet:
      enabled: yes
    rfb:
      enabled: yes
      detection-ports:
        dp: 5900, 5901, 5902, 5903, 5904, 5905, 5906, 5907, 5908, 5909
    mqtt:
      enabled: yes
      # max-msg-length: 1mb
      # subscribe-topic-match-limit: 100
      # unsubscribe-topic-match-limit: 100
      # Maximum number of live MQTT transactions per flow
      # max-tx: 4096
    krb5:
      enabled: yes
    bittorrent-dht:
      enabled: yes
    snmp:
      enabled: yes
    ike:
      enabled: yes
    tls:
      enabled: yes
      detection-ports:
        dp: 443

      # Generate JA3/JA4 fingerprints from client hello. If not specified it
      # will be disabled by default, but enabled if rules require it.
      #ja3-fingerprints: auto
      #ja4-fingerprints: auto

      # What to do when the encrypted communications start:
      # - default: keep tracking TLS session, check for protocol anomalies,
      #            inspect tls_* keywords. Disables inspection of unmodified
      #            'content' signatures.
      # - bypass:  stop processing this flow as much as possible. No further
      #            TLS parsing and inspection. Offload flow bypass to kernel
      #            or hardware if possible.
      # - full:    keep tracking and inspection as normal. Unmodified content
      #            keyword signatures are inspected as well.
      #
      # For best performance, select 'bypass'.
      #
      #encryption-handling: default

    pgsql:
      enabled: no
      # Stream reassembly size for PostgreSQL. By default, track it completely.
      stream-depth: 0
      # Maximum number of live PostgreSQL transactions per flow
      # max-tx: 1024
    dcerpc:
      enabled: yes
      # Maximum number of live DCERPC transactions per flow
      # max-tx: 1024
    ftp:
      enabled: yes
      # memcap: 64mb
    rdp:
      #enabled: yes
    ssh:
      enabled: yes
      #hassh: yes
    http2:
      enabled: yes
      # Maximum number of live HTTP2 streams in a flow
      #max-streams: 4096
      # Maximum headers table size
      #max-table-size: 65536
      # Maximum reassembly size for header + continuation frames
      #max-reassembly-size: 102400
    smtp:
      enabled: yes
      raw-extraction: no
      # Maximum number of live SMTP transactions per flow
      # max-tx: 256
      # Configure SMTP-MIME Decoder
      mime:
        # Decode MIME messages from SMTP transactions
        # (may be resource intensive)
        # This field supersedes all others because it turns the entire
        # process on or off
        decode-mime: yes

        # Decode MIME entity bodies (ie. Base64, quoted-printable, etc.)
        decode-base64: yes
        decode-quoted-printable: yes

        # Maximum bytes per header data value stored in the data structure
        # (default is 2000)
        header-value-depth: 2000

        # Extract URLs and save in state data structure
        extract-urls: yes
        # Scheme of URLs to extract
        # (default is [http])
        #extract-urls-schemes: [http, https, ftp, mailto]
        # Log the scheme of URLs that are extracted
        # (default is no)
        #log-url-scheme: yes
        # Set to yes to compute the md5 of the mail body. You will then
        # be able to journalize it.
        body-md5: no
      # Configure inspected-tracker for file_data keyword
      inspected-tracker:
        content-limit: 100000
        content-inspect-min-size: 32768
        content-inspect-window: 4096
    imap:
      enabled: detection-only
    smb:
      enabled: yes
      detection-ports:
        dp: 139, 445
      # Maximum number of live SMB transactions per flow
      # max-tx: 1024

      # Stream reassembly size for SMB streams. By default track it completely.
      #stream-depth: 0

    nfs:
      enabled: yes
      # max-tx: 1024
    tftp:
      enabled: yes
    dns:
      tcp:
        enabled: yes
        detection-ports:
          dp: 53
      udp:
        enabled: yes
        detection-ports:
          dp: 53
    http:
      enabled: yes

      # Byte Range Containers default settings
      # byterange:
      #   memcap: 100mb
      #   timeout: 60

      # memcap:                   Maximum memory capacity for HTTP
      #                           Default is unlimited, values can be 64mb, e.g.

      # default-config:           Used when no server-config matches
      #   personality:            List of personalities used by default
      #   request-body-limit:     Limit reassembly of request body for inspection
      #                           by http_client_body & pcre /P option.
      #   response-body-limit:    Limit reassembly of response body for inspection
      #                           by file_data, http_server_body & pcre /Q option.
      #
      #   For advanced options, see the user guide


      # server-config:            List of server configurations to use if address matches
      #   address:                List of IP addresses or networks for this block
      #   personality:            List of personalities used by this block
      #
      #                           Then, all the fields from default-config can be overloaded
      #
      # Currently Available Personalities:
      #   Minimal, Generic, IDS (default), IIS_4_0, IIS_5_0, IIS_5_1, IIS_6_0,
      #   IIS_7_0, IIS_7_5, Apache_2
      libhtp:
         default-config:
           personality: IDS

           # Can be specified in kb, mb, gb.  Just a number indicates
           # it's in bytes.
           request-body-limit: 100kb
           response-body-limit: 100kb

           # inspection limits
           request-body-minimal-inspect-size: 32kb
           request-body-inspect-window: 4kb
           response-body-minimal-inspect-size: 40kb
           response-body-inspect-window: 16kb

           # response body decompression (0 disables)
           response-body-decompress-layer-limit: 2

           # auto will use http-body-inline mode in IPS mode, yes or no set it statically
           http-body-inline: auto

           # Decompress SWF files. Disabled by default.
           # Two types: 'deflate', 'lzma', 'both' will decompress deflate and lzma
           # compress-depth:
           # Specifies the maximum amount of data to decompress,
           # set 0 for unlimited.
           # decompress-depth:
           # Specifies the maximum amount of decompressed data to obtain,
           # set 0 for unlimited.
           swf-decompression:
             enabled: no
             type: both
             compress-depth: 100kb
             decompress-depth: 100kb

           # Use a random value for inspection sizes around the specified value.
           # This lowers the risk of some evasion techniques but could lead
           # to detection change between runs. It is set to 'yes' by default.
           #randomize-inspection-sizes: yes
           # If "randomize-inspection-sizes" is active, the value of various
           # inspection size will be chosen from the [1 - range%, 1 + range%]
           # range
           # Default value of "randomize-inspection-range" is 10.
           #randomize-inspection-range: 10

           # decoding
           double-decode-path: no
           double-decode-query: no

           # Can enable LZMA decompression
           #lzma-enabled: false
           # Memory limit usage for LZMA decompression dictionary
           # Data is decompressed until dictionary reaches this size
           #lzma-memlimit: 1mb
           # Maximum decompressed size with a compression ratio
           # above 2048 (only LZMA can reach this ratio, deflate cannot)
           #compression-bomb-limit: 1mb
           # Maximum time spent decompressing a single transaction in usec
           #decompression-time-limit: 100000
           # Maximum number of live transactions per flow
           #max-tx: 512
           # Maximum used number of HTTP1 headers in one request or response
           #headers-limit: 1024

         server-config:

           #- apache:
           #    address: [192.168.1.0/24, 127.0.0.0/8, "::1"]
           #    personality: Apache_2
           #    # Can be specified in kb, mb, gb.  Just a number indicates
           #    # it's in bytes.
           #    request-body-limit: 4096
           #    response-body-limit: 4096
           #    double-decode-path: no
           #    double-decode-query: no

           #- iis7:
           #    address:
           #      - 192.168.0.0/24
           #      - 192.168.10.0/24
           #    personality: IIS_7_0
           #    # Can be specified in kb, mb, gb.  Just a number indicates
           #    # it's in bytes.
           #    request-body-limit: 4096
           #    response-body-limit: 4096
           #    double-decode-path: no
           #    double-decode-query: no

    # Note: Modbus probe parser is minimalist due to the limited usage in the field.
    # Only Modbus message length (greater than Modbus header length)
    # and protocol ID (equal to 0) are checked in probing parser
    # It is important to enable detection port and define Modbus port
    # to avoid false positives
    modbus:
      # How many unanswered Modbus requests are considered a flood.
      # If the limit is reached, the app-layer-event:modbus.flooded; will match.
      #request-flood: 500

      enabled: no
      detection-ports:
        dp: 502
      # According to MODBUS Messaging on TCP/IP Implementation Guide V1.0b, it
      # is recommended to keep the TCP connection opened with a remote device
      # and not to open and close it for each MODBUS/TCP transaction. In that
      # case, it is important to set the depth of the stream reassembling as
      # unlimited (stream.reassembly.depth: 0)

      # Stream reassembly size for modbus. By default track it completely.
      stream-depth: 0

    # DNP3
    dnp3:
      enabled: no
      detection-ports:
        dp: 20000

    # SCADA EtherNet/IP and CIP protocol support
    enip:
      enabled: no
      detection-ports:
        dp: 44818
        sp: 44818

    ntp:
      enabled: yes

    quic:
      enabled: yes

    dhcp:
      enabled: yes

    sip:
      #enabled: yes

# Limit for the maximum number of asn1 frames to decode (default 256)
asn1-max-frames: 256

# Datasets default settings
datasets:
  # Default fallback memcap and hashsize values for datasets in case these
  # were not explicitly defined.
  defaults:
    #memcap: 100mb
    #hashsize: 2048

  rules:
    # Set to true to allow absolute filenames and filenames that use
    # ".." components to reference parent directories in rules that specify
    # their filenames.
    #allow-absolute-filenames: false

    # Allow datasets in rules write access for "save" and
    # "state". This is enabled by default, however write access is
    # limited to the data directory.
    #allow-write: true

##############################################################################
##
## Advanced settings below
##
##############################################################################

##
## Run Options
##

# Run Suricata with a specific user-id and group-id:
#run-as:
#  user: suri
#  group: suri

security:
  # if true, prevents process creation from Suricata by calling
  # setrlimit(RLIMIT_NPROC, 0)
  limit-noproc: true
  # Use landlock security module under Linux
  landlock:
    enabled: no
    directories:
      #write:
      #  - /var/run/
      # /usr and /etc folders are added to read list to allow
      # file magic to be used.
      read:
        - /usr/
        - /etc/
        - /etc/suricata/

  lua:
    # Allow Lua rules. Disabled by default.
    #allow-rules: false

# Some logging modules will use that name in event as identifier. The default
# value is the hostname
#sensor-name: suricata

# Default location of the pid file. The pid file is only used in
# daemon mode (start Suricata with -D). If not running in daemon mode
# the --pidfile command line option must be used to create a pid file.
#pid-file: /var/run/suricata.pid

# Daemon working directory
# Suricata will change directory to this one if provided
# Default: "/"
#daemon-directory: "/"

# Umask.
# Suricata will use this umask if it is provided. By default it will use the
# umask passed on by the shell.
#umask: 022

# Suricata core dump configuration. Limits the size of the core dump file to
# approximately max-dump. The actual core dump size will be a multiple of the
# page size. Core dumps that would be larger than max-dump are truncated. On
# Linux, the actual core dump size may be a few pages larger than max-dump.
# Setting max-dump to 0 disables core dumping.
# Setting max-dump to 'unlimited' will give the full core dump file.
# On 32-bit Linux, a max-dump value >= ULONG_MAX may cause the core dump size
# to be 'unlimited'.

coredump:
  max-dump: unlimited

# If the Suricata box is a router for the sniffed networks, set it to 'router'. If
# it is a pure sniffing setup, set it to 'sniffer-only'.
# If set to auto, the variable is internally switched to 'router' in IPS mode
# and 'sniffer-only' in IDS mode.
# This feature is currently only used by the reject* keywords.
host-mode: auto

# Number of packets preallocated per thread. The default is 1024. A higher number 
# will make sure each CPU will be more easily kept busy, but may negatively 
# impact caching.
#max-pending-packets: 1024

# Runmode the engine should use. Please check --list-runmodes to get the available
# runmodes for each packet acquisition method. Default depends on selected capture
# method. 'workers' generally gives best performance.
#runmode: autofp

# Specifies the kind of flow load balancer used by the flow pinned autofp mode.
#
# Supported schedulers are:
#
# hash     - Flow assigned to threads using the 5-7 tuple hash.
# ippair   - Flow assigned to threads using addresses only.
# ftp-hash - Flow assigned to threads using the hash, except for FTP, so that
#            ftp-data flows will be handled by the same thread
#
#autofp-scheduler: hash

# Preallocated size for each packet. Default is 1514 which is the classical
# size for pcap on Ethernet. You should adjust this value to the highest
# packet size (MTU + hardware header) on your system.
#default-packet-size: 1514

# Unix command socket that can be used to pass commands to Suricata.
# An external tool can then connect to get information from Suricata
# or trigger some modifications of the engine. Set enabled to yes
# to activate the feature. In auto mode, the feature will only be
# activated in live capture mode. You can use the filename variable to set
# the file name of the socket.
unix-command:
  enabled: yes
  filename: /var/run/suricata-command.socket

# Magic file. The extension .mgc is added to the value here.
magic-file: /usr/share/file/magic
#magic-file: 

# GeoIP2 database file. Specify path and filename of GeoIP2 database
# if using rules with "geoip" rule option.
#geoip-database: /usr/local/share/GeoLite2/GeoLite2-Country.mmdb

legacy:
  uricontent: enabled

##
## Detection settings
##

# Set the order of alerts based on actions
# The default order is pass, drop, reject, alert
# action-order:
#   - pass
#   - drop
#   - reject
#   - alert

# Define maximum number of possible alerts that can be triggered for the same
# packet. Default is 15
#packet-alert-max: 15

# Exception Policies
#
# Define a common behavior for all exception policies.
# In IPS mode, the default is drop-flow. For cases when that's not possible, the
# engine will fall to drop-packet. To fallback to old behavior (setting each of
# them individually, or ignoring all), set this to ignore.
# All values available for exception policies can be used, and there is one
# extra option: auto - which means drop-flow or drop-packet (as explained above)
# in IPS mode, and ignore in IDS mode. Exception policy values are: drop-packet,
# drop-flow, reject, bypass, pass-packet, pass-flow, ignore (disable).
exception-policy: auto

# IP Reputation
#reputation-categories-file: /etc/suricata/iprep/categories.txt
#default-reputation-path: /etc/suricata/iprep
#reputation-files:
# - reputation.list

# When run with the option --engine-analysis, the engine will read each of
# the parameters below, and print reports for each of the enabled sections
# and exit.  The reports are printed to a file in the default log dir
# given by the parameter "default-log-dir", with engine reporting
# subsection below printing reports in its own report file.
engine-analysis:
  # enables printing reports for fast-pattern for every rule.
  rules-fast-pattern: yes
  # enables printing reports for each rule
  rules: yes

#recursion and match limits for PCRE where supported
pcre:
  match-limit: 3500
  match-limit-recursion: 1500

##
## Advanced Traffic Tracking and Reconstruction Settings
##

# Host specific policies for defragmentation and TCP stream
# reassembly. The host OS lookup is done using a radix tree, just
# like a routing table so the most specific entry matches.
host-os-policy:
  # Make the default policy windows.
  windows: [0.0.0.0/0]
  bsd: []
  bsd-right: []
  old-linux: []
  linux: []
  old-solaris: []
  solaris: []
  hpux10: []
  hpux11: []
  irix: []
  macos: []
  vista: []
  windows2k3: []

# Defrag settings:

# The memcap-policy value can be "drop-packet", "pass-packet", "reject" or
# "ignore" (which is the default).
defrag:
  memcap: 32mb
  # memcap-policy: ignore
  hash-size: 65536
  trackers: 65535 # number of defragmented flows to follow
  max-frags: 65535 # number of fragments to keep (higher than trackers)
  prealloc: yes
  timeout: 60

# Enable defrag per host settings
#  host-config:
#
#    - dmz:
#        timeout: 30
#        address: [192.168.1.0/24, 127.0.0.0/8, 1.1.1.0/24, 2.2.2.0/24, "1.1.1.1", "2.2.2.2", "::1"]
#
#    - lan:
#        timeout: 45
#        address:
#          - 192.168.0.0/24
#          - 192.168.10.0/24
#          - 172.16.14.0/24

# Flow settings:
# By default, the reserved memory (memcap) for flows is 32MB. This is the limit
# for flow allocation inside the engine. You can change this value to allow
# more memory usage for flows.
# The hash-size determines the size of the hash used to identify flows inside
# the engine, and by default the value is 65536.
# At startup, the engine can preallocate a number of flows, to get better
# performance. The number of flows preallocated is 10000 by default.
# emergency-recovery is the percentage of flows that the engine needs to
# prune before clearing the emergency state. The emergency state is activated
# when the memcap limit is reached, allowing new flows to be created, but
# pruning them with the emergency timeouts (they are defined below).
# If the memcap is reached, the engine will try to prune flows
# with the default timeouts. If it doesn't find a flow to prune, it will set
# the emergency bit and it will try again with more aggressive timeouts.
# If that doesn't work, then it will try to kill the oldest flows using
# last time seen flows.
# The memcap can be specified in kb, mb, gb.  Just a number indicates it's
# in bytes.
# The memcap-policy can be "drop-packet", "pass-packet", "reject" or "ignore"
# (which is the default).

flow:
  memcap: 128mb
  #memcap-policy: ignore
  hash-size: 65536
  prealloc: 10000
  emergency-recovery: 30
  #managers: 1 # default to one flow manager
  #recyclers: 1 # default to one flow recycler thread

# This option controls the use of VLAN ids in the flow (and defrag)
# hashing. Normally this should be enabled, but in some (broken)
# setups where both sides of a flow are not tagged with the same VLAN
# tag, we can ignore the VLAN id's in the flow hashing.
vlan:
  use-for-tracking: true

# This option controls the use of livedev ids in the flow (and defrag)
# hashing. This is enabled by default and should be disabled if
# multiple live devices are used to capture traffic from the same network
livedev:
  use-for-tracking: true

# Specific timeouts for flows. Here you can specify the timeouts that the
# active flows will wait to transit from the current state to another, on each
# protocol. The value of "new" determines the seconds to wait after a handshake or
# stream startup before the engine frees the data of that flow it doesn't
# change the state to established (usually if we don't receive more packets
# of that flow). The value of "established" is the amount of
# seconds that the engine will wait to free the flow if that time elapses
# without receiving new packets or closing the connection. "closed" is the
# amount of time to wait after a flow is closed (usually zero). "bypassed"
# timeout controls locally bypassed flows. For these flows we don't do any other
# tracking. If no packets have been seen after this timeout, the flow is discarded.
#
# There's an emergency mode that will become active under attack circumstances,
# making the engine to check flow status faster. This configuration variables
# use the prefix "emergency-" and work similar as the normal ones.
# Some timeouts doesn't apply to all the protocols, like "closed", for udp and
# icmp.

flow-timeouts:

  default:
    new: 30
    established: 300
    closed: 0
    bypassed: 100
    emergency-new: 10
    emergency-established: 100
    emergency-closed: 0
    emergency-bypassed: 50
  tcp:
    new: 60
    established: 600
    closed: 60
    bypassed: 100
    emergency-new: 5
    emergency-established: 100
    emergency-closed: 10
    emergency-bypassed: 50
  udp:
    new: 30
    established: 300
    bypassed: 100
    emergency-new: 10
    emergency-established: 100
    emergency-bypassed: 50
  icmp:
    new: 30
    established: 300
    bypassed: 100
    emergency-new: 10
    emergency-established: 100
    emergency-bypassed: 50

# Stream engine settings. Here the TCP stream tracking and reassembly
# engine is configured.
#
# stream:
#   memcap: 64mb                # Can be specified in kb, mb, gb.  Just a
#                               # number indicates it's in bytes.
#   memcap-policy: ignore       # Can be "drop-flow", "pass-flow", "bypass",
#                               # "drop-packet", "pass-packet", "reject" or
#                               # "ignore" default is "ignore"
#   checksum-validation: yes    # To validate the checksum of received
#                               # packet. If csum validation is specified as
#                               # "yes", then packets with invalid csum values will not
#                               # be processed by the engine stream/app layer.
#                               # Warning: locally generated traffic can be
#                               # generated without checksum due to hardware offload
#                               # of checksum. You can control the handling of checksum
#                               # on a per-interface basis via the 'checksum-checks'
#                               # option
#   prealloc-sessions: 2048     # 2k sessions prealloc'd per stream thread
#   midstream: false            # don't allow midstream session pickups
#   midstream-policy: ignore    # Can be "drop-flow", "pass-flow", "bypass",
#                               # "drop-packet", "pass-packet", "reject" or
#                               # "ignore" default is "ignore"
#   async-oneside: false        # don't enable async stream handling
#   inline: no                  # stream inline mode
#   drop-invalid: yes           # in inline mode, drop packets that are invalid with regards to streaming engine
#   max-syn-queued: 10          # Max different SYNs to queue
#   max-synack-queued: 5        # Max different SYN/ACKs to queue
#   bypass: no                  # Bypass packets when stream.reassembly.depth is reached.
#                               # Warning: first side to reach this triggers
#                               # the bypass.
#   liberal-timestamps: false   # Treat all timestamps as if the Linux policy applies. This
#                               # means it's slightly more permissive. Enabled by default.
#
#   reassembly:
#     memcap: 256mb             # Can be specified in kb, mb, gb.  Just a number
#                               # indicates it's in bytes.
#     memcap-policy: ignore     # Can be "drop-flow", "pass-flow", "bypass",
#                               # "drop-packet", "pass-packet", "reject" or
#                               # "ignore" default is "ignore"
#     depth: 1mb                # Can be specified in kb, mb, gb.  Just a number
#                               # indicates it's in bytes.
#     toserver-chunk-size: 2560 # inspect raw stream in chunks of at least
#                               # this size.  Can be specified in kb, mb,
#                               # gb.  Just a number indicates it's in bytes.
#     toclient-chunk-size: 2560 # inspect raw stream in chunks of at least
#                               # this size.  Can be specified in kb, mb,
#                               # gb.  Just a number indicates it's in bytes.
#     randomize-chunk-size: yes # Take a random value for chunk size around the specified value.
#                               # This lowers the risk of some evasion techniques but could lead
#                               # to detection change between runs. It is set to 'yes' by default.
#     randomize-chunk-range: 10 # If randomize-chunk-size is active, the value of chunk-size is
#                               # a random value between (1 - randomize-chunk-range/100)*toserver-chunk-size
#                               # and (1 + randomize-chunk-range/100)*toserver-chunk-size and the same
#                               # calculation for toclient-chunk-size.
#                               # Default value of randomize-chunk-range is 10.
#
#     raw: yes                  # 'Raw' reassembly enabled or disabled.
#                               # raw is for content inspection by detection
#                               # engine.
#
#     segment-prealloc: 2048    # number of segments preallocated per thread
#
#     check-overlap-different-data: true|false
#                               # check if a segment contains different data
#                               # than what we've already seen for that
#                               # position in the stream.
#                               # This is enabled automatically if inline mode
#                               # is used or when stream-event:reassembly_overlap_different_data;
#                               # is used in a rule.
#
stream:
  memcap: 64mb
  #memcap-policy: ignore
  checksum-validation: yes      # reject incorrect csums
  #midstream: false
  #midstream-policy: ignore
  inline: auto                  # auto will use inline mode in IPS mode, yes or no set it statically
  reassembly:
    # experimental TCP urgent handling logic
    #urgent:
    #  policy: inline           # drop, inline, oob (1 byte, see RFC 6093, 3.1), gap
    #  oob-limit-policy: drop
    memcap: 256mb
    #memcap-policy: ignore
    depth: 10mb                  # reassemble 1mb into a stream
    toserver-chunk-size: 2560
    toclient-chunk-size: 2560
    randomize-chunk-size: yes
    #randomize-chunk-range: 10
    #raw: yes
    #segment-prealloc: 2048
    #check-overlap-different-data: true

# Host table:
#
# Host table is used by the tagging and per host thresholding subsystems.
#
host:
  hash-size: 4096
  prealloc: 1000
  memcap: 32mb

# IP Pair table:
#
# Used by xbits 'ippair' tracking.
#
#ippair:
#  hash-size: 4096
#  prealloc: 1000
#  memcap: 32mb

# Decoder settings

decoder:
  # Teredo decoder is known to not be completely accurate
  # as it will sometimes detect non-teredo as teredo.
  teredo:
    enabled: true
    # ports to look for Teredo. Max 4 ports. If no ports are given, or
    # the value is set to 'any', Teredo detection runs on _all_ UDP packets.
    ports: $TEREDO_PORTS # syntax: '[3544, 1234]' or '3533' or 'any'.

  # VXLAN decoder is assigned to up to 4 UDP ports. By default only the
  # IANA assigned port 4789 is enabled.
  vxlan:
    enabled: true
    ports: $VXLAN_PORTS # syntax: '[8472, 4789]' or '4789'.

  # Geneve decoder is assigned to up to 4 UDP ports. By default only the
  # IANA assigned port 6081 is enabled.
  geneve:
    enabled: true
    ports: $GENEVE_PORTS # syntax: '[6081, 1234]' or '6081'.

  # maximum number of decoder layers for a packet
  # max-layers: 16

##
## Performance tuning and profiling
##

# The detection engine builds internal groups of signatures. The engine
# allows us to specify the profile to use for them, to manage memory in an
# efficient way keeping good performance. For the profile keyword you
# can use the words "low", "medium", "high" or "custom". If you use custom,
# make sure to define the values in the "custom-values" section.
# Usually you would prefer medium/high/low.
#
# "sgh mpm-context", indicates how the staging should allot mpm contexts for
# the signature groups.  "single" indicates the use of a single context for
# all the signature group heads.  "full" indicates a mpm-context for each
# group head.  "auto" lets the engine decide the distribution of contexts
# based on the information the engine gathers on the patterns from each
# group head.
#
# The option inspection-recursion-limit is used to limit the recursive calls
# in the content inspection code.  For certain payload-sig combinations, we
# might end up taking too much time in the content inspection code.
# If the argument specified is 0, the engine uses an internally defined
# default limit.  When a value is not specified, there are no limits on the recursion.
detect:
  profile: medium
  custom-values:
    toclient-groups: 3
    toserver-groups: 25
  sgh-mpm-context: auto
  inspection-recursion-limit: 3000
  # try to tie an app-layer transaction for rules without app-layer keywords
  # if there is only one live transaction for the flow
  # allows to log app-layer metadata in alert
  # but the transaction may not be the relevant one.
  # guess-applayer-tx: no
  # If set to yes, the loading of signatures will be made after the capture
  # is started. This will limit the downtime in IPS mode.
  #delayed-detect: yes

  prefilter:
    # default prefiltering setting. "mpm" only creates MPM/fast_pattern
    # engines. "auto" also sets up prefilter engines for other keywords.
    # Use --list-keywords=all to see which keywords support prefiltering.
    default: mpm

  # the grouping values above control how many groups are created per
  # direction. Port whitelisting forces that port to get its own group.
  # Very common ports will benefit, as well as ports with many expensive
  # rules.
  grouping:
    #tcp-whitelist: 53, 80, 139, 443, 445, 1433, 3306, 3389, 6666, 6667, 8080
    #udp-whitelist: 53, 135, 5060

  profiling:
    # Log the rules that made it past the prefilter stage, per packet
    # default is off. The threshold setting determines how many rules
    # must have made it past pre-filter for that rule to trigger the
    # logging.
    #inspect-logging-threshold: 200
    grouping:
      dump-to-disk: false
      include-rules: false      # very verbose
      include-mpm-stats: false

# Select the multi pattern algorithm you want to run for scan/search the
# in the engine.
#
# The supported algorithms are:
# "ac"      - Aho-Corasick, default implementation
# "ac-bs"   - Aho-Corasick, reduced memory implementation
# "ac-ks"   - Aho-Corasick, "Ken Steele" variant
# "hs"      - Hyperscan, available when built with Hyperscan support
#
# The default mpm-algo value of "auto" will use "hs" if Hyperscan is
# available, "ac" otherwise.
#
# The mpm you choose also decides the distribution of mpm contexts for
# signature groups, specified by the conf - "detect.sgh-mpm-context".
# Selecting "ac" as the mpm would require "detect.sgh-mpm-context"
# to be set to "single", because of ac's memory requirements, unless the
# ruleset is small enough to fit in memory, in which case one can
# use "full" with "ac".  The rest of the mpms can be run in "full" mode.

mpm-algo: auto

# Select the matching algorithm you want to use for single-pattern searches.
#
# Supported algorithms are "bm" (Boyer-Moore) and "hs" (Hyperscan, only
# available if Suricata has been built with Hyperscan support).
#
# The default of "auto" will use "hs" if available, otherwise "bm".

spm-algo: auto

# Suricata is multi-threaded. Here the threading can be influenced.
threading:
  set-cpu-affinity: no
  # Tune cpu affinity of threads. Each family of threads can be bound
  # to specific CPUs.
  #
  # These 2 apply to the all runmodes:
  # management-cpu-set is used for flow timeout handling, counters
  # worker-cpu-set is used for 'worker' threads
  #
  # Additionally, for autofp these apply:
  # receive-cpu-set is used for capture threads
  # verdict-cpu-set is used for IPS verdict threads
  #
  cpu-affinity:
    - management-cpu-set:
        cpu: [ 0 ]  # include only these CPUs in affinity settings
    - receive-cpu-set:
        cpu: [ 0 ]  # include only these CPUs in affinity settings
    - worker-cpu-set:
        cpu: [ "all" ]
        mode: "exclusive"
        # Use explicitly 3 threads and don't compute number by using
        # detect-thread-ratio variable:
        # threads: 3
        prio:
          low: [ 0 ]
          medium: [ "1-2" ]
          high: [ 3 ]
          default: "medium"
    #- verdict-cpu-set:
    #    cpu: [ 0 ]
    #    prio:
    #      default: "high"
  #
  # By default Suricata creates one "detect" thread per available CPU/CPU core.
  # This setting allows controlling this behaviour. A ratio setting of 2 will
  # create 2 detect threads for each CPU/CPU core. So for a dual core CPU this
  # will result in 4 detect threads. If values below 1 are used, less threads
  # are created. So on a dual core CPU a setting of 0.5 results in 1 detect
  # thread being created. Regardless of the setting at a minimum 1 detect
  # thread will always be created.
  #
  detect-thread-ratio: 1.0
  #
  # By default, the per-thread stack size is left to its default setting. If
  # the default thread stack size is too small, use the following configuration
  # setting to change the size. Note that if any thread's stack size cannot be
  # set to this value, a fatal error occurs.
  #
  # Generally, the per-thread stack-size should not exceed 8MB.
  #stack-size: 8mb

# Luajit has a strange memory requirement, its 'states' need to be in the
# first 2G of the process' memory.
#
# 'luajit.states' is used to control how many states are preallocated.
# State use: per detect script: 1 per detect thread. Per output script: 1 per
# script.
luajit:
  states: 128

# Profiling settings. Only effective if Suricata has been built with
# the --enable-profiling configure flag.
#
profiling:
  # Run profiling for every X-th packet. The default is 1, which means we
  # profile every packet. If set to 1024, one packet is profiled for every
  # 1024 received. The sample rate must be a power of 2.
  #sample-rate: 1024

  # rule profiling
  rules:

    # Profiling can be disabled here, but it will still have a
    # performance impact if compiled in.
    enabled: yes
    filename: rule_perf.log
    append: yes
    # Set active to yes to enable rules profiling at start
    # if set to no (default), the rules profiling will have to be started
    # via unix socket commands.
    #active:no

    # Sort options: ticks, avgticks, checks, matches, maxticks
    # If commented out all the sort options will be used.
    #sort: avgticks

    # Limit the number of sids for which stats are shown at exit (per sort).
    limit: 10

    # output to json
    json: yes

  # per keyword profiling
  keywords:
    enabled: yes
    filename: keyword_perf.log
    append: yes

  prefilter:
    enabled: yes
    filename: prefilter_perf.log
    append: yes

  # per rulegroup profiling
  rulegroups:
    enabled: yes
    filename: rule_group_perf.log
    append: yes

  # packet profiling
  packets:

    # Profiling can be disabled here, but it will still have a
    # performance impact if compiled in.
    enabled: yes
    filename: packet_stats.log
    append: yes

    # per packet csv output
    csv:

      # Output can be disabled here, but it will still have a
      # performance impact if compiled in.
      enabled: no
      filename: packet_stats.csv

  # profiling of locking. Only available when Suricata was built with
  # --enable-profiling-locks.
  locks:
    enabled: no
    filename: lock_stats.log
    append: yes

  pcap-log:
    enabled: no
    filename: pcaplog_stats.log
    append: yes

##
## Netfilter integration
##

# When running in NFQ inline mode, it is possible to use a simulated
# non-terminal NFQUEUE verdict.
# This permits sending all needed packet to Suricata via this rule:
#        iptables -I FORWARD -m mark ! --mark $MARK/$MASK -j NFQUEUE
# And below, you can have your standard filtering ruleset. To activate
# this mode, you need to set mode to 'repeat'
# If you want a packet to be sent to another queue after an ACCEPT decision
# set the mode to 'route' and set next-queue value.
# On Linux >= 3.1, you can set batchcount to a value > 1 to improve performance
# by processing several packets before sending a verdict (worker runmode only).
# On Linux >= 3.6, you can set the fail-open option to yes to have the kernel
# accept the packet if Suricata is not able to keep pace.
# bypass mark and mask can be used to implement NFQ bypass. If bypass mark is
# set then the NFQ bypass is activated. Suricata will set the bypass mark/mask
# on packet of a flow that need to be bypassed. The Netfilter ruleset has to
# directly accept all packets of a flow once a packet has been marked.
#nfq:
#  mode: accept
#  repeat-mark: 1
#  repeat-mask: 1
#  bypass-mark: 1
#  bypass-mask: 1
#  route-queue: 2
#  batchcount: 20
#  fail-open: yes

#nflog support
nflog:
    # netlink multicast group
    # (the same as the iptables --nflog-group param)
    # Group 0 is used by the kernel, so you can't use it
  - group: 2
    # netlink buffer size
    buffer-size: 18432
    # put default value here
  - group: default
    # set number of packets to queue inside kernel
    qthreshold: 1
    # set the delay before flushing packet in the kernel's queue
    qtimeout: 100
    # netlink max buffer size
    max-size: 20000

##
## Advanced Capture Options
##

# General settings affecting packet capture
capture:
  # disable NIC offloading. It's restored when Suricata exits.
  # Enabled by default.
  #disable-offloading: false
  #
  # disable checksum validation. Same as setting '-k none' on the
  # command-line.
  #checksum-validation: none

# Netmap support
#
# Netmap operates with NIC directly in driver, so you need FreeBSD 11+ which has
# built-in Netmap support or compile and install the Netmap module and appropriate
# NIC driver for your Linux system.
# To reach maximum throughput disable all receive-, segmentation-,
# checksum- offloading on your NIC (using ethtool or similar).
# Disabling TX checksum offloading is *required* for connecting OS endpoint
# with NIC endpoint.
# You can find more information at https://github.com/luigirizzo/netmap
#
netmap:
   # To specify OS endpoint add plus sign at the end (e.g. "eth0+")
 - interface: eth2
   # Number of capture threads. "auto" uses number of RSS queues on interface.
   # Warning: unless the RSS hashing is symmetrical, this will lead to
   # accuracy issues.
   #threads: auto
   # You can use the following variables to activate netmap tap or IPS mode.
   # If copy-mode is set to ips or tap, the traffic coming to the current
   # interface will be copied to the copy-iface interface. If 'tap' is set, the
   # copy is complete. If 'ips' is set, the packet matching a 'drop' action
   # will not be copied.
   # To specify the OS as the copy-iface (so the OS can route packets, or forward
   # to a service running on the same machine) add a plus sign at the end
   # (e.g. "copy-iface: eth0+"). Don't forget to set up a symmetrical eth0+ -> eth0
   # for return packets. Hardware checksumming must be *off* on the interface if
   # using an OS endpoint (e.g. 'ifconfig eth0 -rxcsum -txcsum -rxcsum6 -txcsum6' for FreeBSD
   # or 'ethtool -K eth0 tx off rx off' for Linux).
   #copy-mode: tap
   #copy-iface: eth3
   # Set to yes to disable promiscuous mode
   # disable-promisc: no
   # Choose checksum verification mode for the interface. At the moment
   # of the capture, some packets may have an invalid checksum due to
   # the checksum computation being offloaded to the network card.
   # Possible values are:
   #  - yes: checksum validation is forced
   #  - no: checksum validation is disabled
   #  - auto: Suricata uses a statistical approach to detect when
   #  checksum off-loading is used.
   # Warning: 'checksum-validation' must be set to yes to have any validation
   #checksum-checks: auto
   # BPF filter to apply to this interface. The pcap filter syntax apply here.
   #bpf-filter: port 80 or udp
 #- interface: eth3
   #threads: auto
   #copy-mode: tap
   #copy-iface: eth2
   # Put default values here
 - interface: default

# PF_RING configuration: for use with native PF_RING support
# for more info see http://www.ntop.org/products/pf_ring/
pfring:
  - interface: eth0
    # Number of receive threads. If set to 'auto' Suricata will first try
    # to use CPU (core) count and otherwise RSS queue count.
    threads: auto

    # Default clusterid.  PF_RING will load balance packets based on flow.
    # All threads/processes that will participate need to have the same
    # clusterid.
    cluster-id: 99

    # Default PF_RING cluster type. PF_RING can load balance per flow.
    # Possible values are:
    # - cluster_flow:               6-tuple: <src ip, src_port, dst ip, dst port, proto, vlan>
    # - cluster_inner_flow:         6-tuple: <src ip, src port, dst ip, dst port, proto, vlan>
    # - cluster_inner_flow_2_tuple: 2-tuple: <src ip,           dst ip                       >
    # - cluster_inner_flow_4_tuple: 4-tuple: <src ip, src port, dst ip, dst port             >
    # - cluster_inner_flow_5_tuple: 5-tuple: <src ip, src port, dst ip, dst port, proto      >
    # - cluster_round_robin (NOT RECOMMENDED)
    cluster-type: cluster_flow

    # bpf filter for this interface
    #bpf-filter: tcp

    # If bypass is set then the PF_RING hw bypass is activated, when supported
    # by the network interface. Suricata will instruct the interface to bypass
    # all future packets for a flow that need to be bypassed.
    #bypass: yes

    # Choose checksum verification mode for the interface. At the moment
    # of the capture, some packets may have an invalid checksum due to
    # the checksum computation being offloaded to the network card.
    # Possible values are:
    #  - rxonly: only compute checksum for packets received by network card.
    #  - yes: checksum validation is forced
    #  - no: checksum validation is disabled
    #  - auto: Suricata uses a statistical approach to detect when
    #  checksum off-loading is used. (default)
    # Warning: 'checksum-validation' must be set to yes to have any validation
    #checksum-checks: auto
  # Second interface
  #- interface: eth1
  #  threads: 3
  #  cluster-id: 93
  #  cluster-type: cluster_flow
  # Put default values here
  - interface: default
    #threads: 2

# For FreeBSD ipfw(8) divert(4) support.
# Please make sure you have ipfw_load="YES" and ipdivert_load="YES"
# in /etc/loader.conf or kldload'ing the appropriate kernel modules.
# Additionally, you need to have an ipfw rule for the engine to see
# the packets from ipfw.  For Example:
#
#   ipfw add 100 divert 8000 ip from any to any
#
# N.B. This example uses "8000" -- this number must mach the values
# you passed on the command line, i.e., -d 8000
#
ipfw:

  # Reinject packets at the specified ipfw rule number.  This config
  # option is the ipfw rule number AT WHICH rule processing continues
  # in the ipfw processing system after the engine has finished
  # inspecting the packet for acceptance.  If no rule number is specified,
  # accepted packets are reinjected at the divert rule which they entered
  # and IPFW rule processing continues.  No check is done to verify
  # this will rule makes sense so care must be taken to avoid loops in ipfw.
  #
  ## The following example tells the engine to reinject packets
  # back into the ipfw firewall AT rule number 5500:
  #
  # ipfw-reinjection-rule-number: 5500


napatech:
    # When use_all_streams is set to "yes" the initialization code will query
    # the Napatech service for all configured streams and listen on all of them.
    # When set to "no" the streams config array will be used.
    #
    # This option necessitates running the appropriate NTPL commands to create
    # the desired streams prior to running Suricata.
    #use-all-streams: no

    # The streams to listen on when auto-config is disabled or when and threading
    # cpu-affinity is disabled.  This can be either:
    #   an individual stream (e.g. streams: [0])
    # or
    #   a range of streams (e.g. streams: ["0-3"])
    #
    streams: ["0-3"]

    # Stream stats can be enabled to provide fine grain packet and byte counters
    # for each thread/stream that is configured.
    #
    enable-stream-stats: no

    # When auto-config is enabled the streams will be created and assigned
    # automatically to the NUMA node where the thread resides.  If cpu-affinity
    # is enabled in the threading section.  Then the streams will be created
    # according to the number of worker threads specified in the worker-cpu-set.
    # Otherwise, the streams array is used to define the streams.
    #
    # This option is intended primarily to support legacy configurations.
    #
    # This option cannot be used simultaneously with either "use-all-streams"
    # or "hardware-bypass".
    #
    auto-config: yes

    # Enable hardware level flow bypass.
    #
    hardware-bypass: yes

    # Enable inline operation.  When enabled traffic arriving on a given port is
    # automatically forwarded out its peer port after analysis by Suricata.
    #
    inline: no

    # Ports indicates which Napatech ports are to be used in auto-config mode.
    # these are the port IDs of the ports that will be merged prior to the
    # traffic being distributed to the streams.
    #
    # When hardware-bypass is enabled the ports must be configured as a segment.
    # specify the port(s) on which upstream and downstream traffic will arrive.
    # This information is necessary for the hardware to properly process flows.
    #
    # When using a tap configuration one of the ports will receive inbound traffic
    # for the network and the other will receive outbound traffic. The two ports on a
    # given segment must reside on the same network adapter.
    #
    # When using a SPAN-port configuration the upstream and downstream traffic
    # arrives on a single port. This is configured by setting the two sides of the
    # segment to reference the same port.  (e.g. 0-0 to configure a SPAN port on
    # port 0).
    #
    # port segments are specified in the form:
    #    ports: [0-1,2-3,4-5,6-6,7-7]
    #
    # For legacy systems when hardware-bypass is disabled this can be specified in any
    # of the following ways:
    #
    #   a list of individual ports (e.g. ports: [0,1,2,3])
    #
    #   a range of ports (e.g. ports: [0-3])
    #
    #   "all" to indicate that all ports are to be merged together
    #   (e.g. ports: [all])
    #
    # This parameter has no effect if auto-config is disabled.
    #
    ports: [0-1,2-3]

    # When auto-config is enabled the hashmode specifies the algorithm for
    # determining to which stream a given packet is to be delivered.
    # This can be any valid Napatech NTPL hashmode command.
    #
    # The most common hashmode commands are:  hash2tuple, hash2tuplesorted,
    # hash5tuple, hash5tuplesorted and roundrobin.
    #
    # See Napatech NTPL documentation other hashmodes and details on their use.
    #
    # This parameter has no effect if auto-config is disabled.
    #
    hashmode: hash5tuplesorted

##
## Configure Suricata to load Suricata-Update managed rules.
##

default-rule-path: /var/lib/suricata/rules

rule-files:
  - suricata.rules
  - /etc/suricata/rules/*.rules
  - /etc/suricata/rules/*conf
  - ips.rules
  - disable.conf
  - threshold.conf

##
## Auxiliary configuration files.
##

classification-file: /etc/suricata/classification.config
reference-config-file: /etc/suricata/reference.config
threshold-file: /etc/suricata/threshold.config

##
## Include other configs
##

# Includes:  Files included here will be handled as if they were in-lined
# in this configuration file. Files with relative pathnames will be
# searched for in the same directory as this configuration file. You may
# use absolute pathnames too.
#include:
#  - include1.yaml
#  - include2.yaml
